Lab 3 Installing the Motherboard Lab
In the reassembly of the computer we are not going to follow the order recommended in the book.  We will be installing the motherboard first then in order the processor and memory and then the hard drives and CD/DVD drive.
Here is what I want you to do today.
Place the motherboard inside the case. Make sure the ports stick out of the I/O shield at the rear of the case and the screw holes line up with screw holes on the bottom of the case. There should be at least six screw sets, and there might be as many as nine. Use as many screws as there are holes in the motherboard. 

Connect front panel cables to the front panel header. 

Connect any other cables coming from the front panel to the USB and audio ports. 

Install the PSU and connect power cables to the motherboard.